**Levelling stone**

Levelling stone for creating a flat connection surface in round concrete shafts

Enables the creation of a flat connection point for mounting a fitting in a round shaft with the following features:

* Molded block made of special concrete
* Tough concrete reinforced with steel mesh
* Cast-in transport eyelet from nominal size included
* Fastening with special sewage-resistant adhesive
* Special adhesive for concrete shafts included in the scope of delivery

**Levelling stone size (please select):**

**Shaft size:**

* Ø 1000 mm
* Ø 1200 mm
* Ø 1500 mm
* Ø 2000 mm
* Ø 2500 mm
* Ø 3000 mm

**Penstock model:**

* SAFOX©
* CP4
* CP4-RS
* XL4
* XL4-RS

**Opening size:**

* 150 mm
* 200 mm
* 250 mm
* 300 mm
* 400 mm
* 500 mm
* 600 mm
* 700 mm
* 800 mm

**BÜSCH Levelling stone**

or equivalent

**Manufacturer:**

BÜSCH Armaturen Geyer GmbH

Industriestraße 1

09468 Geyer, Germany

Deutschland

[**www.buesch.com**](http://www.buesch.com/)

Quantity........ EUR/ Piece......... EUR/Pos. .........