**Bar screen**

Bar screen to protect penstocks from coarse dirt

Bar screens protect downstream pumps and penstocks from damage caused by coarse dirt with the following features:

* Sturdy welded construction
* Steel grille and frame
* Bar screen for opening\*
* Opening can be locked with padlock provided

(please delete as appropriate)

**Possible penstock installation types:** (please delete as appropriate)

* For lateral doweling into the channel
* For concreting into the prepared channel groove and doweling into the base
* For doweling to the smooth building wall

**Material, bar screen made of:** Stainless steel 1.4301 / 1.4404 / Steel S235JR hot-dip galvanized(please delete as appropriate)

Bar screen size (External dimensions): \_\_\_\_\_\_\_\_\_\_\_\_\_x \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ mm

Bar thickness:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_mm

Grid spacing (bar distance)

Vertical distance\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_mm

Horizontal distance\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_mm

**BÜSCH Bar screen**

or equivalent

**Manufacturer:**

BÜSCH Armaturen Geyer GmbH

Industriestraße 1

09468 Geyer, Germany

Deutschland

[**www.buesch.com**](http://www.buesch.com/)

Quantity........ EUR/ Piece......... EUR/Pos. .........